
**Access box**



**PVC Pipe w/**

**3/8” tubing**

**inside for**

**pump-out**

**Ground level**

**One half of a 55 g drum**

**River Rock / Pebbles**

**5 gal pail**

**Inlet from catch basin**

**PVC 1½” Perforated w/**

**mesh screen over it**

**Figure 1. General schematic of drainage lysimeter construction.**