Aerator Maintenance

Each season all bearing surfaces must be regreased

Grease fittings need to be refilled using a standard grease gun

Grease fittings on each of the brushings in the main frame and the bearings at the end of the rollers should be greased throughout the season as needed.

Inspect Tire pressure

Grease swing arm holders

Check Roller Bearings

Check Wheel Bearings

Check Cotter Pins/Spring Pins to see if need to be replaced